|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Signal name** | **Drive board socket No** | **Pin no. of oscilloscope tube** |  |  |  |
|  | J2 VH6 pin socket | 3SJ1J | 8SJ31J | 7SJ32J | 5SJ38J |
| filament | 1 | 13 | 14 | 12 | 11 |
| filament | 2 | 1 | 1 | 1 | 1 |
| cathode | 3 | 2 | 2 | 2 | 2 |
| Control grid | 4 | 3 | 3 | 3 | 10 |
| Empty foot | 5 |  |  |  |  |
| Focus anode A2 | 6 | 4 | 5 | 4 | 4 |
|  | J6 vh5 pin socket |  |  |  |  |
| First, sanyangji A1, A3 | 1 | 8 | 9 | 8 | 7 |
| Horizontal deflection | 2 | 7 | 10 | 9 | 8 |
| Horizontal deflection | 3 | 6 | 11 | 10 | 3 |
| Vertical deflection | 4 | 9 | 8 | 7 | 6 |
| Vertical deflection | 5 | 10 | 7 | 6 | 9 |

On the drive board, the 5-pin and 6-pin VH sockets are 1 pin near the transformer